|  |
| --- |
| Overview |
| Category Definition |
| Project Presentation |
| Project guidelines |
| Documentation |
| Entry Card attachment |
| Judging Guidelines |
| **Finish** Workmanship should be judged at a high industry standard |
| **Measurements** At least three measurements should be taken at random from project and compared to student notebook drawings. |
| **Student Notebook**Must include step-by-step procedures, working drawing, bill of materials, safety procedures and photos of project while being built |
| **Degree of Difficulty** Should be considered when judging project and points awarded |
| **Welds** No structural welds are to be ground without penalty. Grinding is to be limited to welds that should be ground for functional reasons and/or welds that would normally be ground for cosmetic purposes. Examples: top rails on trailers, fender body outside tops, side latches, etc. may be ground, but frames, cross-members, tongues, filler pipe, etc. are not to be ground. |
|  |  |  |  |  |
| **Judging Points** |  |  |  |  |
| Finish ………………………………………………………………………………………………… | 0-30 points |  |  |
| Measurements…………………………………………………………………………………. | 0-10 points |  |  |
| Student Notebook ……………………………………………………………………………. | 0-40 points |  |  |
| Degree of Difficulty…………………………………………………………………………… | 0-10 points |  |  |
| Welds……………………………………………………………………………………………….. | 0-10 points |  |  |
|  | **Ind.** | **Team** | **Mass** |
| 1 | 2 | 3 |
| **WOOD & METAL - 2800** |
| **Project entries** |  |  |  |  |
|   | 2800 |  |  |  |
| **Metal Projects Chairman will have final decision on category of projects** |  |  |  |